|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | **REPLACEMENT SCHEDULE** | | **Priority Rating** | | |
| **CLASS** | **DESCRIPTION** | **MILES/HOURS** | **YEARS** | **Rating** | **Standard** |
| 003 | Compact/Mid-size Hybrid Sedan | 100,000 | 10 | B1 | Meets standard replacement criteria + 50% |
| 005 | SUV/Cross Over/Mini-Van | 105,000 | 8 | B2 | Meets standard replacement criteria + 40% |
| 006 | Truck, Pickup 1/2 Ton | 110,000 | 8 | B3 | Meets standard replacement criteria + 30% |
| 008 | Truck, Pickup 3/4 Ton | 110,000 | 8 | B4 | Meets standard replacement criteria + 20% |
| 009 | Truck, Utility Body | 110,000 | 8 | B5 | Meets standard replacement criteria + 10% |
| 010 | Sign Posting | 90,000 | 7 | B6 | Meets standard replacement criteria |
| 011 | Truck, Rescue (Airport) | 6,000 Hrs. | 15 | B7 | Not recommended to replace, low usage, may be cheaper to rent. |
| 013 | Truck, 1 Ton | 5,000 Hrs. | 8 |  |  |
| 014 | Truck, Marking | 6,000 Hrs. | 10 |  |  |
| 015 | Truck, Welder | 5,000 Hrs. | 7 |  |  |
| 016 | Truck, Dump 4YD | 6,000 Hrs. | 12 |  |  |
| 016C | Truck, Dump 4YD (CNG) | 6,000 Hrs. | 10 |  |  |
| 018 | Truck, Dump Loader | 6,000 Hrs. | 12 |  |  |
| 018C | Truck, Dump Loader (CNG) | 6,000 Hrs. | 10 |  |  |
| 019 | Truck, Patch | 6,000 Hrs. | 12 |  |  |
| 019C | Truck, Patch (CNG) | 6,000 Hrs. | 10 |  |  |
| 020 | Truck, Fuel Tanker (Airport) | 9,000 Hrs. | 12 |  |  |
| 021 | Truck, Aerial/Stack Bed/Crane | 6,000 Hrs. | 10/12 |  |  |
| 021C | Truck, Aerial/Stack Bed/Crane (CNG) | 6,000 Hrs. | 10 |  |  |
| 023 | Truck, Snow Plow | 6,000 Hrs. | 12 |  |  |
| 024 | Truck, Dump 5YD | 6,000 Hrs. | 12 |  |  |
| 024C | Truck, Dump 5YD (CNG) | 6,000 Hrs. | 12 |  |  |
| 026 | Truck, Drill Rig / Redevelopment Rig | 7,500 Hrs. | 12 |  |  |
| 027 | Truck, Dump 10YD | 7,500 Hrs. | 12 |  |  |
| 027C | Truck, Dump 10YD (CNG) | 7,500 Hrs. | 12 |  |  |
| 028 | Truck, Water (2,500 & 4,000 gallon) | 7,500 Hrs. | 12 |  |  |
| 028C | Truck, Combination (CNG) | 6,000 Hrs. | 10 |  |  |
| 032 | Sweeper, Street (Power Broom) Diesel | 8,000 Hrs. | 12 |  |  |
| 032 | Sweeper, Street (Power Broom) Propane | 5,000 Hrs. | 8 |  |  |
| 032C | Sweeper, Street (Power Broom) (CNG) | 5,000 Hrs. | 8 |  |  |
| 033C | Sweeper, Air (CNG) | 5,000 Hrs. | 8 |  |  |
| 034 | Sweeper, Push Broom | 8,000 Hrs. | 12 |  |  |
| 035 | Sweeper, Bike Path | 8,000 Hrs. | 12 |  |  |
| 037 | Saw, Concrete | ---- | 15 |  |  |
| 038 | Sealer, Crack | 3,000 Hrs. | 10 |  |  |
| 040 | Stump Cutter, Trailer Mounted | 3,000 Hrs. | 12 |  |  |
| 041 | Compressor, Rotary | 3,000 Hrs. | 15 |  |  |
| 047 | Motor Grader | 7,500 Hrs. | 15 |  |  |
| 052 | Roller, Pneumatic | 3,000 Hrs. | 15 |  |  |
| 053 | Roller, Tandem | 2,000 Hrs. | 15 |  |  |
| 061 | Skid Steer | 6,000 Hrs. | 15 |  |  |
| 062 | Tractor, Crawler (>20,000 lbs) | 8,000 Hrs. | 15 |  |  |
| 063 | Tractor, Crawler (20,000-40,000 lbs) | 8,000 Hrs. | 15 |  |  |
| 069 | Tractor, Loader/Backhoe | 6,000 Hrs. | 15 |  |  |
| 071 | Loader, Wheel/Skip Loader | 6,000 Hrs. | 12 |  |  |
| 072 | Loader, Wheel | 6,000 Hrs. | 15 |  |  |
| 073 | Loader, Wheel 2YD Bucket | 6,000 Hrs. | 15 |  |  |
| 078 | Excavator, Truck/Wheel | 8,000 Hrs. | 15 |  |  |
| 082 | Drill Rig | 8,000 Hrs. | 15 |  |  |
| 085 | Mini Truck - All Terrain | ---- | 10 |  |  |
| 092 | Paver | 5,000 Hrs. | 15 |  |  |
| 094 | Truck, Striper | 6,000 Hrs. | 10 |  |  |
| 096 | Chipper, Brush | 3,000 Hrs. | 15 |  |  |
| 098 | Forklift | 5,000 Hrs. | 15 |  |  |